

**Blynk Set up**

Step 1: Create an Account in Blynk

Step 2:



Click on New Template




Step 3 -   
 Type Project name

Select Device as ESP8266

Connection Type – Wfi


Description – optional

Click Done




Click on Devices


Click on New Device




Click on From Template




Click on chose template   
Click on Home Automation




Click on Create


 You can see Api and other header files in Right Corner



Click on edit Dashboard



Select Switch widget



#define BLYNK\_TEMPLATE\_ID "TMPL38W98SAZz"

#define BLYNK\_TEMPLATE\_NAME "Home Automation"

#define BLYNK\_AUTH\_TOKEN "0gNVui8QgId926sVJwGx-oSxNobGe2X-"

